**OH-6A STARTUP CHECKLIST**

1. **BATT SWITCH – ON**
2. **FUEL VALVE - DOWN (OPEN)**
3. **GOV TRIM SWITCH - AFT (DECR) FOR 7 SEC**
4. **STARTER BUTTON - HOLD DOWN**

**Watch N1 RPM increase to 15%**

1. **THROTTLE - TO IDLE**

**Watch N1 RPM stabilise at 60%**

1. **STARTER BUTTON – RELEASE**
2. **GEN SWITCH – ON**
3. **INVERTER SWITCH – ON**
4. **GYRO SWITCH – MAGNETIC**
5. **ADJUST ALTIMETER PRESSURE**
6. **THROTTLE – INCR SLOWLY TO MAX**

**Watch N2 RPM stabilise around 100%**

1. **GOV TRIM SWITCH – ADJ N2 RPM TO 100%**