P-8 Poseidon

CLP_P8


Name: Boeing P-8 Poseidon
Type: maritime patrol and reconnaissance

Crew: Flight: two; Mission: seven
Capacity: 19,800 lb (9,000 kg)
Length: 129 ft 5 in (39.47 m)
Wingspan: 123 ft 6 in (37.64 m)
Height: 42 ft 1 in (12.83 m)
Empty weight: 138,300 lb (62,730 kg)
Max takeoff weight: 189,200 lb (85,820 kg)
Powerplant: 2 × CFM56-7B27A turbofans, 27,300 lbf (121 kN) thrust each

Maximum speed: 564 mph (907 km/h, 490 kn)
Cruise speed: 509 mph (815 km/h, 440 kn)
Combat range: 1,381 mi (2,222 km, 1,200 nmi) ; 4 hours on station (for anti-submarine warfare mission)
Ferry range: 5,200 mi (8,300 km, 4,500 nmi)
Service ceiling: 41,000 ft (12,496 m)
Armament
Hardpoints: 11 total
internal bay with 5 hardpoints and 6 external hardpoints for a variety of conventional weapons, e.g. AGM-84H/K SLAM-ER, AGM-84 Harpoon, Mark 54 torpedo, mines, depth charges, and the High Altitude Anti-Submarine Warfare Weapon Capability (HAAWC) system

Raytheon APY-10 multi-mission surface search radar
AN/ALQ-240 Electronic Support Measures Suite
AN/APS-154 Advanced Airborne Sensor

The P-8 operates in the anti-submarine warfare (ASW), anti-surface warfare (ASUW), and intelligence, surveillance and reconnaissance (ISR) roles

================================
-- from Cowboy's Livery Pack (CLP) by PRCCOWBOY 
================================