JTAC & AWACS for KA-50 & Mi-8 by TurboHog & ProfessorRider (with modifications by Home Fries)


Installation:

This mod is in three parts:
	1) The JTAC & AWACS Main mod
	2) The Ka-50 module-specific mod
	3) the Mi-8 module-specific mod

To use this mod properly, you must have the Main mod enabled.  Then enable the module-specific mods for whichever modules you have installed (i.e. Ka-50/Mi-8).  The reason for the separation is because if you don't have one of the modules (e.g. the Mi-8), installing the Mi-8 file will cause a crash to desktop.



Updating from JTAC Mod 1.5c/DCS World 1.2.16 or earlier:

DCS World 1.5.x and 2.0.x now feature adjustable presets in the Mission Editor, making the R-828/R-863 frequency portions of this mod obsolete.  Please disable and delete the following mod folders:
	JTAC & AWACS R-863 and R-828 Frequencies for Mi-8 (Module)
	JTAC & AWACS R-828 Frequencies for Ka-50 (Module)


Change Log:
1.5	Baseline release for Ka-50 by TurboHog
1.5a	Added ProfessorRider's updates for Mi-8 and Red JTAC
1.5b	Added JSGME separation and DCS World 1.2.14 compatibility
1.5c	DCS World 1.2.15 compatibility
1.5d	1.5.3/2.0.2 compatibility
1.5e	1.5.7/2.1.1 compatibility