#X-55 Profiler Settings

##Stick:

###X-Axis & Y-Axis:
- Deadband: 50
- Curvature: 650
- X-Sat: 1000
- Y-Sat: 1000
- Curve Profile: S
	
###Rudder:
- Deadband: 100 (You may get away with 50, my twist sticks a little)
- Curvature: 650
- X-Sat: 1000
- Y-Sat: 1000
- Curve Profile: S


##Throttle:
###Throttle1 to Rotary4 Axis:
- Deadband: 0
- Curvature: 500
- X-Sat: 1000
- Y-Sat: 1000
- Curve Profile: S