Thanks for trying my x52 Profile!


1. Unzip

2. Move the .pr0 profile to "C:\Users\Public\Documents\SmartTechnology Profiles" and activate it via the Saitek profiler Taskbar icon.

3. Go into any Text editing field and make sure that moving the ministick outputs ",./;" or "ö,-." (depending on your keyboard language) and the precision slider "v"'s and "c"'s.

4. In the DCS options menu click on the controls tab and highlight one of the Saitek x52 key assign fields.

5. Click on "Load Profile" and select the "x52 A10c Input.lua" file.

6. Bind the "HOTAS Speed Brake Switch Aft" command in the DCS Controls menu to the "c" key on your keyboard.

7. Bind the "HOTAS Speed Brake Switch Forward" command to the "v" key on your keyoard.

8. Make sure that your slew controls in the DCS Controls menu are bound to the default keys (,./;). 

9. ENJOY!