Hi all,
This profile is based on DCS-INTERFACE/Exportscripts plugin

To use this profile you need to:
- Install DCS-Interface plugin for StreamDeck. more info here https://forums.eagle.ru/showthread.php?p=4286739

---

GENERAL NOTES: 
- remember to run StreamDeck Software with 'Administration rights' in order to work properly

some commands are based on Keyboard shortcut:
- open/close canopy
- Flash light
- NVG
- Rearm & Refuel
- other functions not related to aircraft such as : briefing, menu radio, Track-ir, kneeboard etc..

--------------

FOLLOWING NOTES ARE VALID ONLY to use the functions for automatic startup 'START 1' and 'START 2' (carrier/field)' THAT ARE BASED ON DCS-BIOS PLUGIN; 
FOR THOSE COMMANDS (that include multiactions, available only with DCS-BIOS plugin) you needo to:
- Install & setup DCS BIOS (https://dcs-bios.readthedocs.io/en/latest/installation.html)
- Install DCS-BIOS plugin for StreamDeck (https://github.com/toureiffel/streamdeck-dcs)

Automatic startup How-To-Use instrucions
- open a F/A-18C COLD&DARK situation
- press START 1
- When RIGHT ENG RPM reaches 25%, then (press RSHIFT+HOME or) move Right thottle from OFF detent to the IDLE detent. R Eng RPM should raise up as normal procedure
- when REng RPM reaches 60-65% you can press START 2 (choose field or carrier button, depending on your situation)
- When LEFT ENG RPM reaches 25%, then (press RALT+HOME or) move Right thottle from OFF detent to the IDLE detent. R Eng RPM should raise up as normal procedure

That is done! 
after START 2 actions completed, you will have INS Switch already set to NAV (and inertial alligment correctly completed, since you choose the right START2 button for your situation Carrier/Field)

(Of course you can customize START-1 and START-2 actions: if you like you can remove/add actions, change order, just do it using streamdeck software)

Now you can go through and..
- Switch int/ext lights as desired
- set FCS
- HSI
etc..


----
THAT IS ALL FOLKS!
Hope you enjoy my profiles!

PVI Maverick
www.pvi.it

