><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> 
Description: This is part of a collection of profiles (A-10C, P-51D & Su-25T). The design principle is to be able to quickly switch from one aircraft to another. 
This is achieved by having the Left MFD as a base for all 3 profiles. When changing aircraft only the Right MFD printout needs to be swapped. This approach has lead to
some compromises and not all "Base" commands will work for all 3 aircraft.
><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> ><> 

><> Installing the SU-25T "Quick Swap" Profile ><>

Step 1: Back up your existing Profile
-------------------------------------
1) Goto Options
2) Goto Controls
3) For "Layer" Select "SU-25T"
4) For each column (e.g. Keyboard, Joystick) select any row and press the "Save Profile As" button.
5) Enter an appropriate name e.g. My_Keyboard.lua, My_Joystick.lua and save in a suitable folder on your computer e.g. c:\DCS World Resources\Backup
6) Select Axis Commands for the "Category" combo box 
7) Goto each completed entry e.g. Column "Joystick - Warthog" and row "Pitch". Press the "Axis Tune" button and write down your values for Deadzone, Saturation X, Saturation Y and Curvature.
--> Loading my profile will overide these settings so if you spent a lot of time getting the feel right for you and want the same after my profile Step 7 is 100% necessary
	
Step 2: Adding a Modifier 
-------------------------
Note: This step is required only once for the 3 profiles (A-10C, Su-25T & P-51D)
1) Goto Options
2) Goto Controls
3) Press the Modifier Button
4) Press Add (Left hand side add button. Right side is for switches)
5) For Device Enter: Joystick - Hotas Warthog...
6) Pull the Joystick Paddle which should then populate the "Select Modifer Button" field.
7) Enter "Pinky" for the "Modifier Button Name". Note: This exact name must be used. 
8) Press OK then OK again.

Step 3: Load my profile
-----------------------
1) Goto Options
2) Goto Controls
3) For "Layer" Select "SU-25T"
4) Select any field in the "Keyboard" Column then press the "Load Profile" button. Select the file "SU-25T-Keyboard.lua"
5) Select any field in the "Joystick - Hotas Warthog" Column then press the "Load Profile" button. Select the file "SU-25T--Joystick.lua"
6) Select any field in the "Throttle - Hotas Warthog" Column then press the "Load Profile" button. Select the file "SU-25T-Throttle.lua"
7) Select any field in the "F16 MFD 1" Column then press the "Load Profile" button. Select the file "SU-25T-MFD1(Left).lua"
8) Select any field in the "F16 MFD 2" Column then press the "Load Profile" button. Select the file "SU-25T-MFD2(Right).lua"
9) [OPTIONAL] Select any field in the "Mouse" Column then press the "Load Profile" button. Select the file "SU-25T-Mouse.lua"
9) [OPTIONAL] Select any field in the "Rudder" Column then press the "Load Profile" button. Select the file "SU-25T-Rudder(Saitek).lua"
10) [OPTIONAL] Select any field in the "TrackIR" Column then press the "Load Profile" button. Select the file "SU-25T-TrackIR.lua"

Step 4: Restore your Axis Settings
----------------------------------
1) Goto Options
2) Goto Controls
3) For "Layer" Select "SU-25T"
4) Select Axis Commands for the "Category" combo box 
5) Goto each completed entry e.g. Column "Joystick - Warthog" and row "Pitch". Press the "Axis Tune" button and enter your preferred values for Deadzone, Saturation X, Saturation Y and Curvature. 
--> If you followed my steps then you should have these values from Step 1 Item 7


Prints outs
-----------
DCS P-51D & Su-25T MFD.pdf
DCS Base Left & A-10C Right MFD.pdf
DCS SU-25T Control Diagram.pdf

Credits: This profile & resources was built upon the work of others ---->
------------------------------------------------------------------------>
Profile Programming Snippets/Inspiration: 					http://forums.eagle.ru/showthread.php?t=92587&highlight=SU-25T+Configuration
Diagram: Developed from excellent document developed for KA-50 by "tietze" 	http://www.digitalcombatsimulator.com/en/files/267607/

NOTE: This profile was developed over a couple of weeks apologies if I have forgotten anyone's contribution.











