Roussen Super Vita Class

ROUSSEN

Type: FACM
Displacement: 580 tons / 668 tons fully loaded
Length: 62 m
Beam: 9.5 m
Draught" 2.6 m
Propulsion: 4 × MTU 16V595 TE90 diesel engines 23,500 hp
Speed: 35 knots (65 km/h; 40 mph)
Complement: 45

Sensors and processing systems:

Thales MW08 3D G-band surveillance radar
Thales Mirador electro-optical target tracker
Thales Scout MkII low probability of intercept radar
Sperry Marine Bridgemaster-E navigation radar
Tacticos combat management system
Aeromaritime IFF Mk12
ICS 2000 integrated communications system

Electronic warfare & decoys:

DR 3000 ESM system
1 SRBOC decoy launcher

Armament:

1 × Oto Melara 76 mm/62 cal.
8 × MM40 Block 2/3 anti-ship missiles
1 × Mk31 21-cell launcher of RAM Block 1 surface-to-air missiles
2 × Oto Melara 30mm cannons