|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 01 | Ground Crew | | | Setup JHMCS | |  |  |
| 02 | HMCS Symbology INT | | | INC | | ↻ | LF |
| 03 | ICP | | | | List | ↓ | CM |
| 04 | ICP – (DED) | | | 0/M-SEL (0/MISC) | | ↓ | CM |
| 05 | ICP – (DED) | | | RCL (R/HMCS) | | ↓ | CM |
| 06 | ICP | | SEQ (HMCS Align) | | | → | CM |
| 07 | ICP - DED | | 0/M-SEL (Coarse) | | |  | CM |
|  | HMCS Cross | | | “Ready” Illuminated | | ☼ | CM |
| 08 | HMCS Cross | | | Align with HUD Cross | |  | CM |
| 09 | HMCS Cross Aligned | | | Radar Cursor / Enable button | | ↓ | CM |
|  | HUD | | | “Aligning” Illuminated | | ☼ | CM |
|  | HUD | | | “Align OK” Illuminated | | ☼ | CM |
| 10 | ICP / DED | 0/M-SEL (Coarse) | | | | ↓ | CM |
|  | DED | AZ/EL auto selected | | | |  | CM |
| 11 | ICP / DED | 0-MSEL (AZ/EL) | | | | ↓ | CM |
|  | HMCS | “FA DX/DY” – Alignment required | | | | ☼ | CM |
| 12 | Radar Cursor | Align Upper Cross to HUD Cross | | | |  | CL/R |
| 13 | ICP | 0-MISC (AZ/EL) | | | | ↓ | CM |
|  | DED | Roll auto selected | | | |  | CM |
| 14 | ICP / DED | 0-MSEL (Roll) | | | | ↓ | CM |
|  | HMCS | “FA Droll” | | | | ☼ | CM |
| 15 | Radar Cursor | Align Lower Cross to Vertical line HUD | | | |  | CM |
| 16 | ICP | 0-MISC (Roll) | | | | ↓ | CM |
|  |  |  | | | |  |  |
|  | END OF PROCEDURE | | | | | |  |
|  |  |