|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | Determine Laser Code | JTAC, Mission Planner | | ↑ | LF |
| 01 | LEFT HDPT | On | | ↑ | RF |
|  | Targeting POD Warm-Up | Est. 3 Mins | |  |  |
| 02 | Master Arm Switch | On | | ↑ | CR |
| 03 | Laser Switch | On | | ↑ | CR |
| 04 | MFD L – TPOD On | FCR / TPG | | ↓ | CL |
| 05 | MFD L - TPOD AG | STBY /A-G | | ↓ | CL |
| 06 | MFD R - SMS Page | Menu / SMS | | ↓ | CR |
| 07 | MFD R - Weapon Select | Select A-G Ordinance CCRP Mode | | ↓ | CR |
| 08 | MDF L - TGP SOI | DMS Down | | ↓ |  |
| 09 | ICP | LIST | | ↓ | CM |
| 10 | ICP / DED | 0 / MISC | | ↓ | CR |
| 11 | ICP / DED | 5 / LASR | | ↓ | CR |
|  | TGP Code will be selected by default |  | |  |  |
| 12 | ICP | Dobber Down | | ↓ | CM |
| 13 | DED LST Code | Enter Code using ICP as desired | | ↓ | CR |
| 14 | ICP | ENTR | | ↓ | CM |
|  | Position aircraft to vicinity of target location | |  |  |  |
| 15 | Laser Spot Search (LSS) Enable | Man Range / Uncage | | ↓ |  |
|  | MFD L – Laser Identified | Laser Spot Track Enabled | |  | CL |
| 16 | MFD L - Lock Target | TMS Up (Point) / TMS Right (Area) | |  | CL |
|  | Complete firing procedure / sequence specific to Ordinance Type | |  |  |  |
| 17 | Laser Spot Search (LSS) Disable | Man Range / Uncage | | ↓ |  |
|  |  |  | |  |  |
|  | END OF PROCEDURE | | | |  |
|  |  |