|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 01 | Master Arm | Simulate | | | | | | | | ↓ | CL |
| GBO | (GBO) GND Jett Enable | | | | Enable | | | | | ↑ | FL |
| 02 | Right HDPT | On | | | | | | | | ↑ | LF |
|  | Allow Est. 3 minutes for Targeting POD to power | | | | | | | | |  |  |
| 03 | ICP | A-G | | | | | | | | ↓ | CM |
| 04 | MFD L – TPOD On | FCR / TPG | | | | | | | | ↓ | CL |
| 05 | MFD L - TPOD AG | STBY /A-G | | | | | | | | ↓ | CL |
| 06 | MFD R - SMS Page | Menu / SMS | | | | | | | | ↓ | CR |
| 07 | MFD R - Weapon Select | AG65D | | | | | | | | ↓ | CR |
| 08 | MFD R – VIS/BORE/PRE | Set to PRE | | | | | | | | ↓ | CR |
| 09 | MFD R – PWR ON/OFF AMG65 | | | | | | | PWR ON | | ↓ | CR |
|  | Allow Est. 5 minutes for AMG65 to power | | | | | | |  | |  |  |
|  | Reposition aircraft in front of boresight target | | | | | | | | |  |  |
| 10 | MFD L – SOI | DMS Down | | | | | | | | ↓ | CL |
| 11 | ICP | Steer Point select | | | | | | | |  |  |
| GBO | MFD L - Snowplow | | | | | | | | CZ /SP |  |  |
| GBO | MFD L - Centre TPOD | | | | | | OVRD x 2 | | | ↓ | CL |
|  | Ground Boresight steps are temp fix to DCS bug with the TPOD SP (26/09/23) | | | | | | | | | |  |
| 12 | MFD L - RDR Cursor Slew | Slew to Boresight Target | | | | | | | | ↓ | CL |
| 13 | MFD L - Lock Boresight Target | | | TMS Up | | | | | | ↓ | CL |
| 14 | MFD R – WPN | Empty OSB Twice / WPN | | | | | | | | ↓ | CR |
| 15 | MFD R – SOI | DMS Down | | | | | | | | ↓ | CR |
| 16 | MFD R - WPN Cursor Slew | Slew to Boresight Target | | | | | | | | ↓ | CR |
| 17 | MFD R - Lock Boresight Target | | TMS Up | | | | | | | ↓ | CR |
|  | Confirm identical targets are locked | | | | | | | | |  |  |
| 18 | MFD R – Boresight | BSGT | | | | | | | | ↓ | CR |
| 19 | NWS A/R DISC MSL Step | Depress to change WPN station | | | | | | | | ↓ |  |
| 20 | Repeat steps 17 – 19 |  | | | | | | | |  |  |
| 21 | MFD R - SMS Page | Menu / SMS | | | | | | | | ↓ | CR |
| GBO | MFD R – PWR ON/ OFF AGM65 | | | PWR OFF | | | | | | ↓ | CR |
| GBO | MFD L – Stow | A-G / STBY | | | | | | | |  | CL |
| GBO | GND Jett Enable | | | | | Disabled | | | | ↓ | FL |
| GBO | Master Arm | Safe | | | | | | | | ↕ | CL |
|  | GBO = Ground Boresight Procedure Only | | | | | | |  | |  |  |
|  | END OF PROCEDURE | | | | | | | | | |  |