|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 01 | Master Arm | | Armed | | | | ↑ | CL |
|  | Right HDPT | | On | | | | ↑ | LF |
|  | Allow Est. 3 minutes for Targeting POD to power | | | | | |  |  |
| 02 | ICP | | A-G | | | | ↓ | CM |
| 03 | MFD R - SMS Page | | Menu / SMS | | | | ↓ | CR |
| 04 | MFD R - Weapon Select | | AG65D | | | | ↓ | CR |
| 05 | MFD R – VIS/BORE/PRE | | Set to VIS | | | | ↓ | CR |
| 06 | MFD R – PWR ON/OFF AMG65 | | | | | PWR ON | ↓ | CR |
| 07 | MFD R – WPN | | | | | Empty OSB Twice / WPN | ↓ | CR |
|  | Allow Est. 5 minutes for AMG65 to power | | | | |  |  |  |
| 08 | HUD – SOI | | DMS Up | | | | ↓ | CL |
|  | Confirm HUD SOI | | Asterisk – Top Left | | | |  |  |
| 09 | HUD - RDR Cursor Slew / Zoom | | | | Slew Seeker ⊡ to Target Area | | ↓ | CL |
| 10 | HUD – Ground Stabilize | | | | TMS Up | | ↓ |  |
|  | Confirm MFD R – SOI | else DMS Down | | | | |  |  |
| 11 | MFD R – RDR Cursor Slew / Zoom | | | | Identify Target | | ↓ | CL |
| 12 | MFD R - Target Lock (within 7nm) | | | TMS Up | | | ↓ | CL |
|  | Note: TMS Down will reset lock, but also set HUD as SOI | | | | | | |  |
|  | MFD R | | | Cross hairs solid / vibrating | | |  |  |
| 13 | Stick | | | Weapon Release | | | ↓ |  |
| 14 | Comm | | | “Rifle” | | |  |  |
|  | Repeat Steps 11 – 14 for subsequent targets | | | | | |  |  |
|  |  | | |  | | |  |  |
|  | END OF PROCEDURE | | | | | | |  |
|  |  |