|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 01 | Master Arm | Armed | | | | | ↑ | CL |
|  | Right HDPT | On | | | | | ↑ | LF |
|  | Allow Est. 3 minutes for Targeting POD to power | | | | | |  |  |
| 02 | ICP | A-G | | | | | ↓ | CM |
| 03 | MFD L – TPOD On | FCR / TPG | | | | | ↓ | CL |
| 04 | MFD L - TPOD AG | STBY /A-G | | | | | ↓ | CL |
| 05 | MFD L - TPOD Auto Handoff | | MAN / AUTO | | | | ↓ | CL |
| 06 | MFD R - SMS Page | Menu / SMS | | | | | ↓ | CR |
| 07 | MFD R - Weapon Select | AG65D | | | | | ↓ | CR |
| 08 | MFD R – VIS/BORE/PRE | Set to PRE | | | | | ↓ | CR |
| 09 | MFD R – PWR ON/OFF AMG65 | | | | | PWR ON | ↓ | CR |
| 10 | MFD R – WPN | | | | | Empty OSB Twice / WPN | ↓ | CR |
|  | Allow Est. 5 minutes for AMG65 to power | | | | |  |  |  |
| 11 | MFD L - SOI | DMS Down | | | | | ↓ | CL |
| 12 | ICP / DED | Select Steer point at Target Area | | | | | ↓ |  |
| 13 | MFD L – TPOD RDR Cursor Slew / Zoom | | | | Identify Target | | ↓ | CL |
| 14 | MFD L - Target Lock (within 7nm) | | | TMS Up | | | ↓ | CL |
|  | MFD R | “Handoff in progress” | | | | |  |  |
|  | MFD R | Cross hairs solid / vibrating | | | | |  |  |
| \* | MFD L - Reattempt failed lock | | | TMS Right | | |  |  |
| 15 | Stick | Weapon Release | | | | |  |  |
| 16 | Com Broadcast | “Rifle” | | | | |  |  |
|  |  | | | |  | |  |  |
|  | END OF PROCEDURE | | | | | | |  |
|  |  |