RQ-4 Global Hawk

CLP_RQ4
CLPRQ4

Name: RQ-4 Global Hawk
Type:  UAV

The RQ-4 Global Hawk is a high-altitude, long-endurance, remotely piloted aircraft with an integrated sensor suite that provides global all-weather, day or night intelligence, surveillance and reconnaissance (ISR) capability.

General Characteristics 
Primary function: high-altitude, long-endurance ISR
Contractor: Northrop Grumman (Prime), Raytheon, L3 Comm 
Power Plant: Rolls Royce-North American F137-RR-100 turbofan engine
Thrust: 7,600 pounds 
Wingspan: 130.9 feet (39.8 meters) 
Length: 47.6 feet (14.5 meters) 
Height: 15.3 feet (4.7 meters) 
Weight: 14,950 pounds (6,781 kilograms) 
Maximum takeoff weight: 32,250 pounds (14628 kilograms) 
Fuel Capacity: 17,300 pounds (7847 kilograms)
Payload: 3,000 pounds (1,360 kilograms) 
Speed: 310 knots (357 mph) 
Range: 12,300 nautical miles 
Endurance:  more than 34 hours
Ceiling: 60,000 feet (18,288 meters) 
Armament: None
Crew (remote): three (LRE pilot, MCE pilot, and sensor operator) 

================================
-- from Cowboy's Livery Pack (CLP) by PRCCOWBOY 
================================
