|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | FIRE CONTROL RADAR DESIGNATED | |  | |  |  |
| 01 | ICP – Mode Select | | A-G Mode | | ↓ | CM |
| 02 | MFD L - FCR SOI | | DMS Down | |  | CL |
|  | Verify SOI box on MFD L | |  | |  | CL |
| 03 | MFD L - Radar Mode | | GM / GMT | | ↓ | CL |
| 04 | MFD L - RDR Cursor | | Slew / Zoom to target | |  | CL |
| 05 | MFD L - Lock Target | | TMS Up | |  | CL |
| 06 | ICP - CNI Page | | Dobber Left (RTN) | | ← | CM |
| 07 | ICP – Mark Page | | Mark (7) | | ↓ | CL |
|  | Verify Mark \*FCR \* | |  | |  | CM |
| 08 | DED - Store Mark Point | | TMS Up | |  | CM |
|  |  | |  | |  |  |
|  | TARGETING POD DESIGNATED | |  | |  |  |
| 01 | ICP – Mode Select | | A-G Mode | | ↓ | CM |
| 02 | MFD L - TGP SOI | | DMS Down | |  | CL |
|  | Verify SOI box on MFD L | |  | |  | CL |
| 03 | MFD L - RDR Cursor | | | Slew / Zoom to target |  | CL |
| 04 | MFD L - Lock Target | | TMS Up -Point / TMS Right - Area | |  | CL |
| 05 | ICP - CNI Page | | Dobber Left (RTN) | | ← | CM |
| 06 | ICP – Mark Page | | Mark (7) | | ↓ | CM |
|  | Verify MARK \*TGP \* | |  | |  | CM |
| 07 | DED - Store Mark Point | | TMS Up | |  | CM |
|  |  | |  | |  |  |
|  | HUD / HMCS DESIGNATED | |  | |  |  |
| 01 | HUD - SOI | | DMS UP | | ↓ | CL |
|  | Verify SOI \* on HUD Top Left | |  | |  | CM |
| 02 | ICP - CNI Page | | Dobber Left (RTN) | | ← | CM |
| 03 | ICP – Mark Page | | Mark (7) | |  | CM |
|  | Verify MARK \*HUD \* | |  | |  | CM |
| 04 | Velocity Vector | | Coarse align with target | |  | CM |
| 05 | Designation Circle - Stabilize | | TMS Up | |  | CM |
| 06 | Designation Circle | Fine align with RDR cursor switch | | |  | CM |
| 07 | DED - Store Mark Point | TMS Up | | |  | CM |
|  | *Note: Steerpoint #26 – 30 reserved for Mark Points in Database* | | | |  |  |
|  | END OF PROCEDURE | | | | |  |
|  |  |